KbdGetStatus

Bindings:

C:

typedef struct _KBDINFO { /* kbst */ USHORT cb; /* length in bytes of this structure */ USHORT fsMask; /* bit mask of functions to be altered */ USHORT chTurnAround; /* define TurnAround character */ USHORT fsInterim; /* interim character flags */ USHORT fsState; /* shift states */ }KBDINFO; #define INCL_KBD USHORT rc = KbdGetStatus(Structure, KbdHandle); PKBDINFO Structure; /* Data structure */ HKBD KbdHandle; /* Keyboard handle */ USHORT rc; /* return code */

MASM:

KBDINFO struc kbst_cb dw ? ;length in bytes of this structure kbst_fsMask dw ? ;bit mask of functions to be altered kbst_chTurnAround dw ? ;define TurnAround character kbst_fsInterim dw ? ;interim character flags kbst_fsState dw ? ;shift states KBDINFO ends EXTRN KbdGetStatus:FAR INCL_KBD EQU 1 PUSH@ OTHER Structure ;Data structure PUSH WORD KbdHandle ;Keyboard handle CALL KbdGetStatus Returns WORD

This call gets the current state of the keyboard.

KbdGetStatus (StatData, KbdHandle)

StatData (PKBDINFO) - output Address of the keyboard status structure:

length (USHORT) Length, in bytes, of this data structure, including length.

10	Only valid value.

sysstate (USHORT) State as follows:

Bit	Description
15-9	Reserved, set to zero.
8	Shift return is on.
7	Length of the turn-around character (meaningful only if bit 6 is on).
6	Turn-around character is modified.
5	Interim character flags are modified.
4	Shift state is modified.
3	ASCII mode is on.
2	Binary mode is on.
1	Echo off.
0	Echo on.

turnchardef (USHORT) Definition of the turn-around character. In ASCII and extended-ASCII format, the turn-around character is defined as the carriage return. In ASCII format only, the turn-around character is defined in the low-order byte.

intcharflag (USHORT) Interim character flags:

Bit	Description
15-8	NLS shift state.
7	Interim character flag is on.
6	Reserved, set to zero.
5	Application requested immediate conversion.
4-0	Reserved, set to zero.

shiftstate (USHORT) Shift state as follows:

Bit	Description
15	SysReq key down
14	CapsLock key down
13	NumLock key down
12	ScrollLock key down
11	Right Alt key down
10	Right Ctrl key down
9	Left Alt key down
8	Left Ctrl key down
7	Insert on
6	CapsLock on
5	NumLock on
4	ScrollLock on
3	Either Alt key down
2	Either Ctrl key down
1	Left Shift key down
0	Right Shift key down.

KbdHandle (HKBD) - input Default keyboard or the logical keyboard.

rc (USHORT) - return Return code descriptions are:

0	NO_ERROR
376	ERROR_KBD_INVALID_LENGTH
439	ERROR_KBD_INVALID_HANDLE
445	ERROR_KBD_FOCUS_REQUIRED
447	ERROR_KBD_KEYBOARD_BUSY
464	ERROR_KBD_DETACHED
504	ERROR_KBD_EXTENDED_SG

Remarks

The initial state of the keyboard is established by the system at application load time. Some default states may be modified by the application through KbdSetStatus. KbdGetStatus returns only those keyboard parameters initially set by KbdSetStatus. The returned parameters are:

Input Mode

Interim Character Flags

Shift State

Echo State

Turnaround Character

KbdGetStatus completes only when the handle has access to the physical keyboard (focus) or the handle is 0 and no other handle has the focus.

Family API Considerations

Some options operate differently in the DOS mode than in the OS/2 mode. Therefore, the following restrictions apply to KbdGetStatus when coding in the DOS mode:

Interim character is not supported

TurnAround character is not supported

NLS_SHIFT_STATE is always NULL.

KbdHandle is ignored.