Note: This IBM PC BIOS API call is for DOS/Win16 personality only. Use Family API for portability.

Note: osFree Macro Library provides macros for most of functions

@CharPeek

Brief

BIOS Interrupt

INT16H: 01H

Family API

fapi

Syntax

@CharPeek

Parameters

none

Return

none